
Georeferencing:

Upper left geographic: 177d17'32.31" W; 66d54'22.82" N
Lower right geographic: 62d32'49.65" W; 34d18'05.61" N
Upper left geocoded: -2600000.000 E; 10500000.000 N
Lower right geocoded: 3100000.000 E; 5700000.000 N
True origin: 95d00'00.0000"W; 0d00'00.0000"N
Pixel Information: Each pixel value is contained in a 2-byte (16-bit unsigned integer); 
pixel size, 
horizontal resolution: 1000m; pixel size, 
vertical resolution: 1000m
Image Size: 5700 pixels x 4800 lines 
Format_Name: binary

Map_Projection_Name: Lambert Conformal Conic
1st Standard Parallel: 49 
2nd Standard Parallel: 77
Longitude_of_Central_Meridian: -95
Latitude_of_Projection_Origin: 0
False_Easting:   0.000
False_Northing: 0.000
Geodetic_Model:
Horizontal_Datum_Name: NAD83
Ellipsoid_Name: GRS 1980
