Scotian Margin (Mariprobe) 2001 - Line 2

Pos.	Instrument	Deployment
longitude	Deployment
latitude	Deployment
depth	Recovery
longitude	Recovery
latitude	Clock reset
(JD:hh:mm)	Clock check
(JD:hh:mm)	Clock drift
(msec)	Drift rate
(msec/hour)	Raw data files	Remarks	
1	DAL-N	62.780191°W	44.186295°N	240 m	62.778871°W	44.187667°N	171:15:00	178:12:32	+3.093	+0.02	000-234	Static shift: -2.413msec 1) 	
2	DAL-M	62.485631°W	43.891325°N	149 m	62.483028°W	43.893185°N	172:00:20	178:14:32	+1.987	+0.01	000-238	Static shift: +3.588 msec 1) 	
3	DAL-D	62.194519°W	43.595477°N	98 m	62.192041°W	43.595367°N	172:00:05	178:16:15	+3.672	+0.02	000-242	Static shift: +0.145 msec 1) 	
4	DAL-C	61.914466°W	43.307676°N	644 m	61.911990°W	43.307979°N	172:03:22	178:18.11	-7.159	-0.05	000-245	Static shift: -1.892 msec 1) 	
5	GSC-1	61.684533°W	43.068345°N	131 m	-	-	171:21:56	-			-	Static shift: -2.085 msec 1) 	
6	GSC-2	61.558802°W	42.936681°N	860 m	61.558319°W	42.932475°N	172:01:11	~179:00:30	-10.430	-0.06	000-511	Static shift: +0.688 msec 1) 	
7	GSC-3	61.391300°W	42.760178°N	1977 m	61.390165°W	42.760473°N	172:03:55	~179:04:30	-601.152	Jump or drift?	000-265	Static shift: +2.052 msec 1) 	
8	DAL-B	61.263013°W	42.624359°N	2660 m	61.257702°W	42.625841°N	172:05:57	179:06:30	+20.621	+0.12	000-269	Static shift: +3.345 msec 1) 	
9	DAL-A	61.119012°W	42.469692°N	3447 m	61.117204°W	42.469988°N	172:11:40	179:08:40	+8.121	+0.05	000-266	Static shift: +2.381 msec 1) 	
10	DAL-H	60.986284°W	42.326812°N	3727 m	60.993978°W	42.326812°N	172:13:46	179:11:13	-8.317	-0.05	000-278	Static shift: +1.002 msec 1) 	
11	DAL-I	60.846161°W	42.175860°N	3978 m	60.851016°W	42.176335°N	172:16:36	179:13:52	+10.696	+0.06	000-283	Static shift: +0.923 msec 1) 	
12	DAL-E	60.709662°W	42.027860°N	4052 m	60.717373°W	42.026323°N	172:18:06	179:16:29	+3.733	+0.02	000-289	Static shift: +1.985 msec 1) 	
13	GSC-4	60.606182°W	41.915191°N	4251 m	60.622189°W	41.910139°N	172:08:32	~179:19:00	-16.748	-0.09	000-293	Static shift: +3.810 msec 1) 	
14	GSC-5	60.500629°W	41.799626°N	4432 m	60.508872°W	41.798674°N	172:12:14	~179:21:15	+90.549	+0.51	000-298	Static shift: +1.052 msec 1) 	
15	GCS-6	60.369140°W	41.655018°N	4588 m	60.372090°W	41.653673°N	172:23:32	~179:23:45	+24.357	+0.14	000-303	Static shift: +2.195 msec 1) 	
16	GSC-8	60.235464°W	41.506835°N	4698 m	60.239610°W	41.504475°N	173:01:19	~180:02:30	-23.000	-0.14	000-308	Static shift: -2.170 msec 1) 	
17	DAL-G	60.103637°W	41.360182°N	4778 m	60.110407°W	41.361687°N	172:22:19	180:05:24	-3.716	-0.02	000-313	Static shift: -0.784 msec 1) 	
18	DAL-J	59.971800°W	41.212324°N	4838 m	59.977192°W	41.212690°N	172:12:00	180:08:03	+21.157	+0.11	000-318	Static shift: -0.513 msec 1) 	
19	DAL-L	59.835981°W	41.059144°N	4881 m	59.843440°W	41.059725°N	173:01:47	180:11:00	-5.045	-0.03	000-312	Static shift: -2.070 msec 1) 	
20	DAL-K	59.662480°W	40.861689°N	4935 m	59.672575°W	40.852678°N	173:07:19	180:14:05	+7.474	+0.04	000-318	Static shift: -1.449 msec 1) 	
21	DAL-F	59.499970°W	40.676986°N	5005 m	59.508038°W	40.668833°N	173:05:59	180:16:48	-68.764	-0.38	000-323	Static shift: +2.710 msec 1) 	

Sampling rate
GSC / Dalhousie instruments		139.00 Hz
GSC-2				278.00 Hz

Instruments
GSC = Geological Survey of Canada (Atlantic Division)	three-component 4.5-Hz geophones + hydrophone
DAL = Dalhousie University (Dept. of Oceanography)		three-component 4.5-Hz geophones + hydrophone

Clock drift
+ sign	OBS clock is ahead of GPS clock
- sign	OBS clock is behind GPS clock
 1) There is an additional static shift of +2 ms for all instruments