Scotian Margin (Mariprobe) 2001 - Line 3

Pos.	Instrument	Deployment
longitude	Deployment
latitude	Deployment
depth	Recovery
longitude	Recovery
latitude	Clock reset
(JD:hh:mm)	Clock check
(JD:hh:mm)	Clock drift
(msec)	Drift rate
(msec/hour)	Raw data files	Remarks	
1	GSC-2	64.433635°W	40.619351°N	4347 m	64.451033°W	40.622817°N	187:19:57	190:19:48	-1.201	-0.02	000-087	Static shift: +2.031 msec 1) 	
2	GSC-3	64.556138°W	40.794147°N	4112 m	64.567846°W	40.801305°N	187:20:22	190:22:22	+8.709	+0.12	000-092	Static shift: +0.788 msec 1) 	
3	GSC-4	64.680299°W	40.968122°N	3851 m	64.683338°W	40.970804°N	187:21:27	191:00:50	-9.755	-0.13	000-096	Static shift: +3.603 msec 1) 	
4	DAL-K	64.805426°W	41.143577°N	3548 m	64.805426°W	41.149651°N	187:18:12	191:03:19	+10.653	+0.13	000-099	Static shift: +2.052 msec 1) 	
5	DAL-H	64.931394°W	41.316956°N	3189 m	64.926807°W	41.321401°N	187:18:27	191:05:16	-5.477	-0.07	000-102	Static shift: +0.127 msec 1) 	
6	DAL-G	65.058282°W	41.490906°N	2810 m	65.055705°W	41.492508°N	187:18:34	191:07:08	+5.473	+0.06	000-106	Static shift: -3.199 msec 1) 	
7	GSC-5	65.185863°W	41.664520°N	2379 m	65.187119°W	41.664761°N	187:22:33	191:08:59	+39.255	+0.48	000-111	Static shift: -1.456 msec 1) 	
8	GSC-6	65.315322°W	41.838529°N	1926 m	65.310990°W	41.842455°N	187:23:04	191:11:10	+13.325	+0.16	000-115	Static shift: +0.366 msec 1) 	
9	GSC-8	65.444803°W	42.012148°N	1180 m	65.454144°W	42.006809°N	188:00:04				No data	Static shift: +1.795 msec 1) 	
10	DAL-B	65.576042°W	42.185408°N	112 m	65.584332°W	42.186137°N	187:18:48	191:14:32	+9.068	+0.10	000-121	Static shift:+3.509  msec 1) 	
11	DAL-J	65.707947°W	42.358811°N	102 m	65.705380°W	42.362026°N	188:12:41	191:16:00	+8.629	+0.11	000-125	Static shift: -2.740 msec 1) 	
12	DAL-I	65.859456°W	42.555196°N	80 m	65.861733°W	42.556234°N	187:19:04	191:17:06	+5.209	+0.06	000-127	Static shift: +1.816 msec 1) 	

Sampling rate
GSC / Dalhousie instruments		139.00 Hz

Instruments
GSC = Geological Survey of Canada (Atlantic Division)	three-component 4.5-Hz geophones + hydrophone
DAL = Dalhousie University (Dept. of Oceanography)		three-component 4.5-Hz geophones + hydrophone

Clock drift
+ sign	OBS clock is ahead of GPS clock
- sign	OBS clock is behind GPS clock

1)  There is an additional static shift of +2 ms for all instruments